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Solid Hardwood Overhead Coiling Doors

PART  1   GENERAL
SECTION INCLUDES
Wood Slat Overhead Coiling Doors.
Accessories.

RELATED SECTIONS
01 00 00 General Requirements
05 41 00 Structural Metal Stud Framing
06 11 00 Wood Framing
06 20 00 Finish Carpentry
08 01 33 Operation and Maintenance of Coiling Doors and Grilles
08 06 10 Door Schedule
08 06 71 Door Hardware Schedule
08 33 00 Coiling Doors and Grilles
08 71 00 Door Hardware
09 06 00 Schedules for Finishes

REFERENCES 
APA The Engineered Wood Association (APA), PR-N124
EPA TSCA Title VI PART 770 Formaldehyde standards for composite wood products 08-28-26
EPA Document Number: 815R24006 Human Health Toxicity Assessment for Perfluorooctanoic Acid (PFOA) and Related Salts April 2024
CARB Approval to use No-added Formaldehyde Resins by Composite Wood Product Manufacturers under section 93120.3, title 17, California Code of Regulations.
LEED® for Building Design and Construction V4
2026 International Building Code (IBC): Sections 104.2.3 Alternative materials, design and methods of construction and equipment.
2026 International Building Code (IBC): Section 104.11 Alternative materials, design and methods of construction and equipment.
2026 International Residential Code (IRC): Sections R104.2.2 Alternative materials, design and methods of construction and equipment.
2026 International Residential Code (IRC): Section R104.11 Alternative materials, design and methods of construction and equipment.
ISO 21930:2017 Sustainability in Building and Civil Engineering works – Core Rules for environmental Product Declaration of Construction Products and Services.


[bookmark: _Hlk196141841]SUBMITTALS
Submit under provisions of Section 01 33 23 Shop Drawings, Product Data and Samples.
Manufacturer's data sheets on each product to be used, including:
Preparation instructions and recommendations.
Storage and handling requirements and recommendations.
Installation methods.

QUALITY ASSURANCE
Overhead Coiling Doors manufacturer will maintain quality standards for all materials used on the project. 
Overhead Coiling Doors will adhere to all relevant industry standards and regulations to ensure that materials meet or exceed performance and safety requirements.
Manufacturer will qualify their material suppliers to maintain high-quality materials.

DELIVERY, STORAGE, AND HANDLING
Store off the ground, well supported, on a flat well-drained surface.
Do not store doors in areas with standing water. 
Factory packaging is not waterproof, store all materials inside the building. 
Follow manufacturer’s instructions on removal of packaging. 
Restrict access by other trades to protect doors before installation and until accepted by the owner. 
Keep products clean and dry. Inspect prior to installation.

PROJECT CONDITIONS
Install Overhead Coiling Doors only when the building is secure and weather tight. 

WARRANTY
[bookmark: _Hlk138762513]See section 01 70 00 Execution and Closeout Requirements, for additional warranty requirements.
Provide manufacturer's standard warranty. 
Duration of limited warranty to be as follows:
Manufacturer to provide a limited lifetime warranty to the original retail purchaser that the overhead coiling doors, when properly installed and maintained, will be free from defects in workmanship, construction, and materials.
Warranty will exclude normal wear and tear. 
Motorized roll up doors will have a five-year warranty on the motor.
Installer to provide a one-year warranty covering installation defects. 


COORDINATION
Installer to coordinate with other trades to maintain jobsite safety during door installation.

PART  2   PRODUCTS
[bookmark: _Hlk137722466]MANUFACTURERS
Basis of Design; Woodfold Mfg., Inc.1811 18th Avenue, Forest Grove, OR 97116, Phone: 503-357-7181, Solid Hardwood rollup doors series 801-802-803-804 Website: https://woodfold.com/, Email: architects@woodfold.com or woodfold@woodfold.Com
See drawings for sizes, locations and types of different Solid Hardwood Overhead Coiling Doors.
Install Overhead Coiling Doors as shown on the drawings.

OPERATION OF DOORS
See plans for door operation. 
For manual operation manufacturer will provide standard pulls.
For crank operation standard manufacturers systems will be used.
For motorized operation manufacturer will provide standard wiring diagram.
Locks and latches are not to be used on motorized roll up doors. 
Motor operation will use a tubular system.
Motorized doors will have manual override capability.
Latching or locking of manual and crank operated overhead coiling doors to be shown on the hardware schedule.

PRODUCT INFORMATION
Individual slats to be interconnected using plastic coated, aerospace grade stainless steel cables fixed at the top and bottom of door.

SUSTAINABLE ATTRIBUTES
Sustainable Attributes.
Wood used in rollup doors to meet requirements of: EPA TSCA Title VI 40 CFR 770.17 No-added formaldehyde resins.
CARB ATCM 93120.3(c) Special Provision for Manufacturers of HWPW, PB and MDF with No-Added Formaldehyde Based Resins
Engineered-wood components of doors to be compliant with CDPH/EHLB Standard Method for the Testing and Evaluation of Volatile Organic Chemical Emissions.
Antimicrobial (non-arsenic). Overhead Coiling Doors to be designed for use in buildings that are properly maintained to avoid moisture infiltration, condensation and/or accumulation at wall surfaces, particularly in warm, humid climates.
Compliant with California, Proposition 65
Overhead Coiling Doors are to certify they are PFOA free, that they do not contain, nor will Overhead Coiling Doors degrade to, Perfluoro Octanoic Acid. (PFOA)
Materials and Resources – MR Credit - Leadership Extraction Practices.
Recycled Content.
Steel components – Default 25% Post-Consumer recycle content.
Aluminum components- 40.6% Post-Industrial/Pre-Consumer & 13.6%
Post-Consumer recycled content (per Aluminum Extruders Council EPD).
Precise recycle content and weights of components to be provided once order is finalized.

HARDWOOD SPECIES
Architect to select wood species from Northern Red Oak, White Oak, Eastern Maple, Natural Birch, African Mahogany, or American Cherry.

HARDWOOD COILING DOORS FINISH
Wood sections are to be factory finished before assembly.
Architect to select wood finish.
Architect will provide finish required for hardwood coiling doors.
For jobsite finishing of hardwood doors see section 09 91 00 Painting.

MOCK UP
If required by the architect Overhead Coiling Door manufacturer will work with the architect to design an onsite mockup.
Material and installation costs to be billed to the general contractor.

PART  3   EXECUTION
EXAMINATION
Material to be inspected for shipping damage.
Damaged material to be replaced before Overhead Coiling Door installation begins
PART  4   INSTALLATION
INSTALLATION
Manufacture to provide 3” course thread wood screws.
For installation to substrates other than wood fasteners are to be supplied by others.
Overhead Coiling Doors to be installed by factory approved installers.
Installer to provide owner with an optional service contract for the Overhead Coiling Doors. 

SITE INSPECTION
Installer to verify opening sizes before partitions are ordered.
Installer to verify wall construction meets the requirements of the specifications.
Notify architect of any wall construction that does not meet project requirements.
Do not proceed with installation until wall defects are corrected.

CARE AND MAINTENANCE
Manufacturer to provide owner with written instructions for the care and maintenance of Overhead Coiling Doors.
Installer will provide one training session with building maintenance staff.
Training will cover proper use and maintenance of Overhead Coiling Doors.

JOBSITE WASTE REMOVAL
See Section 01 74 00 Cleaning and Waste Management.
Boxes and wrapping will be removed from the building and placed in onsite waste containers.
Onsite disposal container by others. 

PROTECTION
Overhead Coiling Doors to be protected from damage by other trades. 
END OF SECTION 
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